------------------- ePass2003 Software Developer's Kit ----------------------

[Version Information]
    Model        : ePass2003
    COS          : V1.0 
    SDK          : V1.1
    Middleware   : 1.1.13.401
    Release Date : 2013.04.16
    Language     : English


[Product Information]

    1.  Product Model: 
        ePass2003

    2.  Default Password
        SOPIN    :  entersafe
        User PIN :  12345678

    3.  Quick Start Procedure
	
        a) Install middleware in 		   
           \PKI\Redist\ePass2003-Setup.exe
		
        b) Download certificate with manager tool (Optional)
           \PKI\Utilities\ePassManagerAdm_2003.exe

		   
[Release Note]

  1. Support Microsoft Smart Card Mini Driver
  
  2. Add secure desktop feature
	
	3. Support PKCS#11 v2.20 standard
	
	4. Support Windows 2000/XP/2003/Vista/2008/7/8, Linux and MacOS X
	
	5. Support all 64bits Windows system
	
	6. If only use PKCS#11 interface, it is no need to install the middleware. 
	    The application can call PKCS#11 library directly.

	   
[General Introduction]
	
	The PKI, also known as Public Key Infrastructure, is adopted widely in 
	strong authentication applications. Due to sensitive data, such as private
	keys, are very important to the PKI system, high security smart cards are
	normally selected as the carrier to perform the role.
	
	FEITIAN ePass2003 is a high security PKI based USB token incorporating the most 
	powerful cryptograhpic technology and standards available today. It is designed 
	for all Public Key Infrastructure environments and brings two-factor cryptographic 
	authentications to applications where security is critical. FIPS 140-2 validated 
	card operating system and on-board key management mechanism enable a higher level 
	of security assurance to a wide range of sensitive applications. With the combined 
	compatibility of Microsoft Minidriver and OpenSC, the ePass2003 is compatible with 
	applications running on Windows, Linux and Mac and therefore is the ideal choice for 
	all industries requiring high level protection such as government, enterprise, financial 
	institutions and media companies. 
	   	   
[Product Features]

    * High-performance CPU chip
    * FIPS 140-2 Level 2 Certified
    * Card Operating System with proprietary IP - FEITIAN COS
    * Onboard RSA 1024/2048 key generation
    * Support RSA, DES, 3DES AES, SHA-1 and SHA-2 and ECDSA(optional) algorithms
    * 64bits universal unique hardware serial number
    * Hardware implemented random number generator
    * 64KB memory space
    * USB driverless device
    * Fully support PKI application. Support MS CAPI,CNG and PKCS#11 API
    * Support Microsoft Smart Card Minidriver and OpenSC
    * Provide standard middleware API (CSP and PKCS#11)
    * Support storing multiple keys
    * Hardware implemented digital signature
    * Support X.509v3 format certificate
    * Seamlessly integration with PKI applications, such as Internet Explorer, 
	  Outlook, Outlook Express, Firefox etc.
    
	
[Supported Platforms]

    	
    Windows 2000
    windows XP (32bit & 64bit)
    Windows 2003 (32bit & 64bit)
    Windows Vista (32bit & 64bit)
    Windows 2008 (32bit & 64bit)
    Windows 7 (32bit & 64bit)
    Windows 8 (32bit & 64bit)
    
    Linux 
    
    MacOS X


 